   		D-Link IEEE802.1x supplicant Program

    The Supp1x Program supports the functionality of IEEE802.1x supplicant.
    Supp1x allow you to authenticate with IEEE802.1x-ready ethernet switch.
    The authentication type supported right now is MD5-Challenge.
    Supp1x can run on Windows 98, Windows 98SE, Windows ME, Windows 2000,
    and Windows XP.

    To install Supp1x, run the Setup.exe program.


    NOTE: The supplicant function is build in by Windows XP, if you want
          to use Supp1x in Windows XP, please turn off the supplicant
          function of your Windows XP.