; SoundMAX device information file for ODM
; Analog Devices, Inc. Copyright(c) 1998 - 2003

[Version]
Signature="$CHICAGO$"
Class=MEDIA
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
provider=%ANLG%
DriverVer = 06/02/2003,%DriverBuildID%
CatalogFile=smx.cat

[ControlFlags]
ExcludeFromSelect = *

[Manufacturer]
%MfgName%=AnalogDevices

[AnalogDevices]
%*WDM_AC97AUD.DeviceDesc%=WDM_JS_JE, pci\ven_8086&dev_24D5&subsys_53754144
%*WDM_AC97AUD.DeviceDesc%=WDM_JS_JE, pci\ven_8086&dev_24D5&subsys_A0001458
%*WDM_AC97AUD.DeviceDesc%=WDM_JS_JE, pci\ven_8086&dev_24D5&subsys_75801462
%*WDM_AC97AUD.DeviceDesc%=WDM_JS_JE, pci\ven_8086&dev_24D5&subsys_218814A4
%*WDM_AC97AUD.DeviceDesc%=WDM_P411,  pci\ven_8086&dev_24D5&subsys_00951071
%*WDM_AC97AUD.DeviceDesc%=WDM_ASUS,  pci\ven_8086&dev_24D5&subsys_80F31043

[DestinationDirs]
DefaultDestDir = 10,system32\drivers   ; %SystemRoot%\system32\drivers
WDM_AC97AUD.CopyList = 10,system32\drivers   ; %SystemRoot%\system32\drivers
DevUpgrd-Files = 10, win9xmig\DevUpgrd
W2KDriver-Files = 10, win9xmig\DevUpgrd\ADIW2K
Sensaura = 10, system32
Stubfile = 10, system32\drivers	;;wdmstub

[WDM_JS_JE]
DriverVer = 06/02/2003,%DriverBuildID%
AlsoInstall=ks.registration(ks.inf),wdmaudio.registration(wdmaudio.inf)
CopyFiles=WDM_AC97AUD.CopyList, DevUpgrd-Files, W2KDriver-Files, Stubfile					;;wdmstub
DelReg=WDM_AC97AUD.DelReg, DriverInfo.DelReg
AddReg=WDM_AC97AUD.AddReg, WDM_AC97AUD_GUID.AddReg, DriverInfo.AddReg, Js_Je.AddReg, Js_JeO.AddReg, SPDIF.AddReg, DevUpgrd-AddReg
KnownRegEntries=ICHAUD.KnownRegEntries

[WDM_P411]
DriverVer = 06/02/2003,%DriverBuildID%
AlsoInstall=ks.registration(ks.inf),wdmaudio.registration(wdmaudio.inf)
CopyFiles=WDM_AC97AUD.CopyList, DevUpgrd-Files, W2KDriver-Files, Stubfile					;;wdmstub
DelReg=WDM_AC97AUD.DelReg, DriverInfo.DelReg
AddReg=WDM_AC97AUD.AddReg, WDM_AC97AUD_GUID.AddReg, DriverInfo.AddReg, Js_Je.AddReg, Js_JeP.AddReg, SPDIF.AddReg, DevUpgrd-AddReg
KnownRegEntries=ICHAUD.KnownRegEntries

[WDM_ASUS]
DriverVer = 06/02/2003,%DriverBuildID%
AlsoInstall=ks.registration(ks.inf),wdmaudio.registration(wdmaudio.inf)
CopyFiles=WDM_AC97AUD.CopyList, DevUpgrd-Files, W2KDriver-Files, Stubfile					;;wdmstub
DelReg=WDM_AC97AUD.DelReg, DriverInfo.DelReg
AddReg=WDM_AC97AUD.AddReg, WDM_AC97AUD_GUID.AddReg, DriverInfo.AddReg, Js_Je.AddReg, Js_JeA.AddReg, SPDIF.AddReg, DevUpgrd-AddReg
KnownRegEntries=ICHAUD.KnownRegEntries

[DevUpgrd-AddReg]
HKLM,"Software\Microsoft\Windows\CurrentVersion\Setup\Migration DLLs","Microsoft Device Upgrade Pack",,%10%\win9xmig\DevUpgrd
HKLM,%Upgd%,"pci\ven_8086&dev_2415",,%10%\%UpDir%
HKLM,%Upgd%,"pci\ven_8086&dev_2425",,%10%\%UpDir%
HKLM,%Upgd%,"pci\ven_8086&dev_2445",,%10%\%UpDir%
HKLM,%Upgd%,"pci\ven_8086&dev_2485",,%10%\%UpDir%
HKLM,%Upgd%,"pci\ven_8086&dev_24C5",,%10%\%UpDir%
HKLM,%Upgd%,"pci\ven_8086&dev_24D5",,%10%\%UpDir%
HKLM,%Upgd%,"pci\ven_8086&dev_7195",,%10%\%UpDir%
HKLM,%Upgd%,"pci\ven_1106&dev_3058",,%10%\%UpDir%
HKLM,%Upgd%,"pci\ven_1106&dev_3059",,%10%\%UpDir%
HKLM,%Upgd%,"pci\ven_10DE&dev_01B1",,%10%\%UpDir%
HKLM,%Upgd%,"pci\ven_10DE&dev_006A",,%10%\%UpDir%
HKLM,%Upgd%,"pci\ven_10DE&dev_00DA",,%10%\%UpDir%
HKLM,%Upgd%,"pci\ven_10B9&dev_5451",,%10%\%UpDir%
HKLM,%Upgd%,"pci\ven_1039&dev_7012",,%10%\%UpDir%
HKLM,%Upgd%,"pci\ven_1022&dev_746D",,%10%\%UpDir%
HKLM,%Upgd%,"pci\ven_1022&dev_4341",,%10%\%UpDir%

[DevUpgrd-Files]
Migrate.dll

[W2KDriver-Files]
smwdm4C5.inf
smwdm.sys
a3d.dll
smsens.sys  ;;Sensaura
aeaudio.sys ;;Andrea

[ICHAUD.KnownRegEntries]
IsWin98Gold=keep

[IsWin98Gold]
1=HKLM,Software\Microsoft\Windows\CurrentVersion,VersionNumber,0,4.10.1998

[WDM_JS_JE.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%, AC97Aud.Interface.Topology
AddInterface=%ANDREA_INTERFACE%,,AC97Aud.Interface.Andrea

[WDM_P411.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%, AC97Aud.Interface.Topology
AddInterface=%ANDREA_INTERFACE%,,AC97Aud.Interface.Andrea

[WDM_ASUS.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%, AC97Aud.Interface.Topology
AddInterface=%ANDREA_INTERFACE%,,AC97Aud.Interface.Andrea

;Begin Andrea Win9x

[WDM_JS_JE.HW]
AddReg=FilterAddReg

[WDM_P411.HW]
AddReg=FilterAddReg

[WDM_ASUS.HW]
AddReg=FilterAddReg

[WDM_AC97AUD.DelReg]
HKR, Drivers
HKR, Disable
HKR, Settings

[WDM_AC97AUD.AddReg]
HKR,,AssociatedFilters,,"wdmaud,swmidi,redbook"
HKR,,Driver,,smwdm.sys
HKR,,NTMPDriver,,"wdmstub.sys,smwdm.sys,sbemul.sys"	;;wdmstub

HKR,Drivers,SubClasses,,"wave,midi,mixer"

HKR,Drivers\wave\wdmaud.drv, Driver,,wdmaud.drv
HKR,Drivers\midi\wdmaud.drv, Driver,,wdmaud.drv
HKR,Drivers\mixer\wdmaud.drv,Driver,,wdmaud.drv

HKR,Drivers\wave\wdmaud.drv, Description,,%*WDM_AC97AUD.DeviceDesc%
HKR,Drivers\midi\wdmaud.drv, Description,,%WDM_MIDI%
HKR,Drivers\mixer\wdmaud.drv,Description,,%*WDM_AC97AUD.DeviceDesc%

; Establish max/min values for Volume nodes. "xxxxMax" is the setting for
;  maximum volume level (minimum attenuation). "xxxxMin" is the setting for
;  minimum volume level (maximum attenuation). These values are the Max/Min
;  bits written to the register for the Max/Min level. As an example, the
;  MicIn maximum volume can be set to 2 which equals a maximum output of +9 db,
;  the MicIn minimum is set to 10 which equals a minimum output of - 12 db.
;  (All register values are Hex.)

HKR, Settings, "HP_VMax", 1, 06   ;   Headphone Volume
HKR, Settings, "MicVMax", 1, 02   ;   Mic In Volume
HKR, Settings, "MicVMin", 1, 10   ;
HKR, Settings, "FntVMax", 1, 08   ;   Front Volume
HKR, Settings, "SurVMax", 1, 08   ;   Surround Volume
HKR, Settings, "CtrVMax", 1, 08   ;   Center Volume
HKR, Settings, "LfeVMax", 1, 08   ;   Lfe Volume ( sub woofer )

; Max/Min record levels. xxxRMax is the maximum gain code for that record
;  source. xxxRMin is the minimum gain code for that source.

; Default volume / mute settings. These are the initial installation settings.
; The volume default values are tested againts the Max/Min values that may have
;  been previously established. The Boolean settings (Mute, 20 db, etc.) are
;  set as 0 = FALSE, non-zero = TRUE;
;
; Note that a particular hardware platform may not implement all signal paths.
;
; This is the mixed digital PCM stream (Wave, SW Synth and Digital Redbook)
; This setting is not adjustable from a Mixer control slider. This is
; not adjustable from the Mixer applet.
HKR, Settings, "PCMOutVolume", 1, 08 ;   PCM Out volume 8 = 0db gain, 7 = +1.5db
HKR, Settings, "NULL", 1, 00     ;   Generic handler for un-named nodes

HKR, Settings, "MasV", 1, 08     ;   Master Volume
HKR, Settings, "MasM", 1, 00     ;   Master Mute

HKR, Settings, "PCBV", 1, 08     ;   PCBeep Volume
HKR, Settings, "PCBM", 1, 00     ;   PCBeep Mute
                                    
HKR, Settings, "PhoV", 1, 08     ;   Phone Volume
HKR, Settings, "PhoM", 1, 00     ;   Phone Mute
HKR, Settings, "LinV", 1, 08     ;   LineIn Volume
HKR, Settings, "LinM", 1, 00     ;   LineIn Mute
HKR, Settings, "VidV", 1, 08     ;   Video Volume
HKR, Settings, "VidM", 1, 00     ;   Video Volume
HKR, Settings, "AuxV", 1, 08     ;   Aux Volume
HKR, Settings, "AuxM", 1, 00     ;   Aux Mute

HKR, Settings, "MicV", 1, 08     ;   Mic In Volume
HKR, Settings, "MicM", 1, 01     ;   Mic In Mute
HKR, Settings, "MicS", 1, 00     ;   Mic In Select (0 == Mic1, 1 == Mic2)

HKR, Settings, "ACDV", 1, 08     ;   Analog CD Volume (not digital redbook !)
HKR, Settings, "ACDM", 1, 00     ;   Analog CD Mute
HKR, Settings, "EnableRecordMuting", 1, 01 ; Mute Record when slider at bottom.
HKR, Settings, "P3DV", 1, 0A     ;   Stereo Wide (Phat 3D) Volume ( 0 - F )
HKR, Settings, "P3DM", 1, 00     ;   Phat 3D Mute
HKR, Settings, "P3DB", 1, 01     ;   Use enhancement on digital streams
HKR, Settings, "MicBoostVal", 1, 12 ; AD1981A Microphone Boost. 00 = +20db, 01 = +10db, 02 = +30db, 12 = +30db on and +10db off
HKR, Settings, "CalPin", 1, 1F   ; Disables calibration
HKR, Settings, "MonV", 1, 08     ;   Mono Out Volume
HKR, Settings, "MonM", 1, 00     ;   Mono Out Mute
HKR, Settings, "RecS", 1, 00     ;   Record source (0=Mic, 1=CD, 2=Vid, 3=Aux
                                 ;      4=LineIn, 5=WaveOut, 6=MonoOut, 7=Phone
HKR, Settings, "HP_V", 1, 08     ;   Headphone Volume
HKR, Settings, "HP_M", 1, 00     ;   Headphone Mute

HKR, Settings, "FntV", 1, 08     ;   Surround Volume
HKR, Settings, "FntM", 1, 00     ;   Surround Mute
HKR, Settings, "SurV", 1, 08     ;   Surround Volume
HKR, Settings, "SurM", 1, 00     ;   Surround Mute
HKR, Settings, "CtrM", 1, 00     ;   Center Mute
HKR, Settings, "LfeV", 1, 08     ;   Lfe Volume ( sub woofer )
HKR, Settings, "LfeM", 1, 00     ;   Lfe Mute ( sub woofer )

HKR, Settings, "BB_V", 1, 08     ;   BassBoost Level ( 0 -> 0xF )
HKR, Settings, "BB_M", 1, 00     ;   BassBoost Mute
HKR, Settings, "VRefDisable", 1, 00 ;  AD1981A VRefDisable. 00 = enable, 01 = disable
HKR, Settings, "VRefLevel", 1, 00   ;  AD1981A VRefLevel. 00 = 2.25v, 01 = 3.7v
HKR, Settings, "EnableSpeakerEQ", 1, 01 ;  AD198x Speaker EQ. 00 = Disable EQ, 01 = Enable EQ
HKCU,Software\Microsoft\Multimedia\Audio,DefaultFormat,,"Default Quality"
HKCU,Software\Microsoft\Multimedia\Audio\WaveFormats,"Default Quality",1, 01,00,01,00,22,56,00,00,44,AC,00,00,02,00,10,00

; Record Controls

HKR, Settings, "MicR", 1, 08     ;   Mic
HKR, Settings, "OutR", 1, 00     ;   Line output loopback
HKR, Settings, "ACDR", 1, 01     ;   CD (Analog CD, not Redbook Audio)
HKR, Settings, "VidR", 1, 01     ;   Video
HKR, Settings, "AuxR", 1, 01     ;   Aux
HKR, Settings, "LinR", 1, 01     ;   Line In
HKR, Settings, "MonR", 1, 01     ;   Mono output loopback
HKR, Settings, "PhoR", 1, 01     ;   Phone
;Apply for AD198x codecs.  Ability to swap control and data.
HKR, Disable, "SWPC",               1, 00 ; control enabled
HKR, Settings, "MagicNumber",       1, 00, 30, 00, 60
HKR, Settings, "SwapCenterLFE",     1, 02 ; Swap the data when the control is swapped
;Apply 3DB boost to streams processed by SM2/3
HKR, Settings, "3dBBoost", 1, 01, 00, 00, 00
; Enable Interrupt on each processed BDL
;  00 = Interrupt only when KMixer request
;  01 = Interrupt on every BDL
HKR, Settings, "SGUpdate", 1, 01

; Disable Node display on mixer applet. Set to 00 to enable, 01 to disable.
HKR, Disable, "NULL", 1, 00     ;   Generic handler for un-named nodes
HKR, Disable, "PCBV", 1, 00     ;   PCBeep Volume
HKR, Disable, "PCBM", 1, 00     ;   PCBeep Mute
HKR, Disable, "PhoV", 1, 00     ;   Phone Volume
HKR, Disable, "PhoR", 1, 00     ;   Phone Volume
HKR, Disable, "PhoM", 1, 00     ;   Phone Mute
HKR, Disable, "VidV", 1, 00     ;   Video Volume
HKR, Disable, "VidM", 1, 00     ;   Video Mute
HKR, Disable, "20db", 1, 00     ;   Mic 20db Gain
HKR, Disable, "MicV", 1, 00     ;   Mic In Volume
HKR, Disable, "MicM", 1, 00     ;   Mic In Mute

HKR, Disable, "ACDV", 1, 00     ;   Analog CD Volume (not digital redbook !)
HKR, Disable, "ACDM", 1, 00     ;   Analog CD Mute
HKR, Disable, "P3DV", 1, 00     ;   Stereo Wide (Phat 3D) Volume
HKR, Disable, "P3DM", 1, 00     ;   Phat 3D Mute
HKR, Disable, "P3DB", 1, 00     ;   Phat 3D Bypass for digital streams
HKR, Disable, "MonV", 1, 00     ;   Mono Out Volume
HKR, Disable, "MonM", 1, 00     ;   Mono Out Mute

HKR, Disable, "FntV", 1, 00     ;   Front Volume
HKR, Disable, "FntM", 1, 00     ;   Front Mute
HKR, Disable, "SurV", 1, 00     ;   Surround Volume
HKR, Disable, "SurM", 1, 00     ;   Surround Mute
HKR, Disable, "CtrV", 1, 00     ;   Center Volume
HKR, Disable, "CtrM", 1, 00     ;   Center Mute
HKR, Disable, "LfeV", 1, 00     ;   Lfe Volume ( sub woofer )
HKR, Disable, "LfeM", 1, 00     ;   Lfe Mute ( sub woofer )

; Record Controls
HKR, Disable, "MicR", 1, 00     ;   Mic
HKR, Disable, "ACDR", 1, 00     ;   CD (Analog CD, not Redbook Audio)
HKR, Disable, "VidR", 1, 00     ;   Video
HKR, Disable, "OutR", 1, 00     ;   Line output loopback
HKR, Disable, "MonR", 1, 00     ;   Mono output loopback
HKR, Disable, "BB_V", 1, 00     ;   BassBoost Level
HKR, Disable, "BB_M", 1, 00     ;   BassBoost Mute
HKR, Disable, "Voice", 1, 01    ;   ICHx MicIn DMA channel. 00 = enable, 01 = disable.
;If you want the MonoOut to track the Master Volume control, set MonoWithMaster
;to 01. If you want separate Master Volume and MonoOut controls, set
;MonoWithMaster to 00. If MonoWithMaster = 01, the "MonoOut" controls will _not_
;be present on SndVol32 (the Master Volume control will control the MonoOut
;output)
HKR, Settings, "MonoWithMaster", 1, 00 ;   00 = Normal, 01 = MonoOut tracks Master

;If a AD1885/6 is detected and you want the (headphone) amplifier to track the
;Master Volume control, set HPWithMaster to 01 (same code written to Master
;Volume and Headphone volume based upon Master volume settings). If you want
;separate controls for the Master Volume and Headphone, set HPWithMaster to 00.
;If ;HpWithMaster = 01, the "Headphone" controls will _not_ be present on
;SndVol32 (the Master Volume control will control the Headphone amplifier output)
;If HpWithMaster = 01, the following INF settings are ignored, HP_VMax, HP_VMin,
;HP_V, HP_M, HP_P.
;An AD1887 uses the settings for the Master Volume to control the output and
;automatically sets HPWithMaster.
HKR, Settings, "HPWithMaster", 1, 01 ;   00 = Normal, 01 = Amplifier output tracks Master

;If a AD1885/6 is detected and the (headphone) amplifier is used, set HP_P to 00.
;If the amplified output is not used, set HP_P to 01. If you selected
;HPWithMaster, this setting is interpreted to be 01 (not active).
HKR, Disable, "HP_P", 1, 00     ;   Headphone Pin (Headphone destination on AD1885/6)
                                ;    00 = active, 01 = not active

[SPDIF.AddReg]
; Enable/Disable the S\PDIF channel
HKR, Disable, "SPDF", 1, 00     ;   01 = Disabled (default), 00 = Enabled
; S/PDIF channel Data Type
HKR, Settings, "CAC3",  1, 01   ;   00 = AC3 not checked (default), 01 = AC3 checked
HKR, Settings, "CPCM",  1, 01   ;   00 = PCM not checked (default), 01 = PCM checked

[Js_Je.AddReg]
; Jack Sharing + Jack Enumeration
HKR, Disable,  "MicS",             1, 00 ; Mic In Select
HKR, Settings, "JackSense",	   1, 50, 00, 00, 00
HKR, Settings, "JackSense2",	   1, F0, 02, 00, 00
HKR, Settings, "JackSenseConf",	   1, 11, 20, F5, FF
HKR, Settings, "JackSenseInhibit", 1, F1, FF, FF, FF
HKR, Settings, "JackSenseShare",   1, FF, 57, FF, FF

[Js_JeO.AddReg]
HKR, Settings, "CtrV",        1, 08 ; Center Volume
HKR, Settings, "StereoMic",   1, 01 ; 00 = mono mic support, 01 = stereo mic support
HKR, Settings, "SWPC",        1, 00 ; Controls not swapped

[Js_JeP.AddReg]
HKR, Settings, "CtrV",        1, 08 ; Center Volume
HKR, Settings, "StereoMic",   1, 00 ; 00 = mono mic support, 01 = stereo mic support
HKR, Settings, "SWPC",        1, 00 ; Controls not swapped

[Js_JeA.AddReg]
HKR, Settings, "ACDRMAX",     1, 0A ; CD (Analog CD, not Redbook Audio)
HKR, Settings, "AuxRMAX",     1, 0A ; Aux
HKR, Settings, "CtrV",        1, 00 ; Center Volume
HKR, Settings, "LinRMAX",     1, 0A ; Line In
HKR, Settings, "LockMSToOMS", 1, 01 ; Causes left/right swap of stereo microphone input when OMS bit is set.
HKR, Settings, "SPDIFBit",    1, 00 ; Always set the Copy Protection Bit to 0
HKR, Settings, "StereoMic",   1, 01 ; 00 = mono mic support, 01 = stereo mic support
HKR, Settings, "SWPC",        1, 01 ; Controls not swapped

[WDM_AC97AUD_GUID.AddReg]
HKLM,%MediaCategories%\%ADIGUID.PcBeep%,Name,,%Pin.PcBeep%
HKLM,%MediaCategories%\%ADIGUID.PcBeep%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.Phone%,Name,,%Pin.Phone%
HKLM,%MediaCategories%\%ADIGUID.Phone%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.Video%,Name,,%Pin.Video%
HKLM,%MediaCategories%\%ADIGUID.Video%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.MonoOut%,Name,,%Pin.MonoOut%
HKLM,%MediaCategories%\%ADIGUID.MonoOut%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.BBoost%,Name,,%Pin.BBoost%
HKLM,%MediaCategories%\%ADIGUID.BBoost%,Display,1,00,00,00,00

HKLM,%MediaCategories%\%ADIGUID.PCBeepVol%,Name,,%Control.PCBeepVol%
HKLM,%MediaCategories%\%ADIGUID.PCBeepVol%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.PhoneVol%,Name,,%Control.PhoneVol%
HKLM,%MediaCategories%\%ADIGUID.PhoneVol%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.VIDVol%,Name,,%Control.VIDVol%
HKLM,%MediaCategories%\%ADIGUID.VIDVol%,Display,1,00,00,00,00

HKLM,%MediaCategories%\%ADIGUID.20DB%,Name,,%Control.20DB%
HKLM,%MediaCategories%\%ADIGUID.20DB%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.PHATBypass%,Name,,%Control.PHATBypass%
HKLM,%MediaCategories%\%ADIGUID.PHATBypass%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.MonoVol%,Name,,%Control.MonoVol%
HKLM,%MediaCategories%\%ADIGUID.MonoVol%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.MicSelect%,Name,,%Control.MicSelect%
HKLM,%MediaCategories%\%ADIGUID.MicSelect%,Display,1,00,00,00,00

HKLM,%MediaCategories%\%ADIGUID.CaptureVid%,Name,,%Control.CaptureVid%
HKLM,%MediaCategories%\%ADIGUID.CaptureVid%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.CaptureMono%,Name,,%Control.CaptureMono%
HKLM,%MediaCategories%\%ADIGUID.CaptureMono%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.CapturePhone%,Name,,%Control.CapturePhone%
HKLM,%MediaCategories%\%ADIGUID.CapturePhone%,Display,1,00,00,00,00

HKLM,%MediaCategories%\%ADIGUID.Front%,Name,,%Pin.Front%
HKLM,%MediaCategories%\%ADIGUID.Front%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.Surround%,Name,,%Pin.Surround%
HKLM,%MediaCategories%\%ADIGUID.Surround%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.Center%,Name,,%Pin.Center%
HKLM,%MediaCategories%\%ADIGUID.Center%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.Lfe%,Name,,%Pin.Lfe%
HKLM,%MediaCategories%\%ADIGUID.Lfe%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.FrontVol%,Name,,%Control.FrontVol%
HKLM,%MediaCategories%\%ADIGUID.FrontVol%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.SurroundVol%,Name,,%Control.SurroundVol%
HKLM,%MediaCategories%\%ADIGUID.SurroundVol%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.CenterVol%,Name,,%Control.CenterVol%
HKLM,%MediaCategories%\%ADIGUID.CenterVol%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.LfeVol%,Name,,%Control.LfeVol%
HKLM,%MediaCategories%\%ADIGUID.LfeVol%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.BBoostVol%,Name,,%Control.BBoostVol%
HKLM,%MediaCategories%\%ADIGUID.BBoostVol%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.SwapC%,Name,,%Control.SwapC%
HKLM,%MediaCategories%\%ADIGUID.SwapC%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.SwapD%,Name,,%Control.SwapD%
HKLM,%MediaCategories%\%ADIGUID.SwapD%,Display,1,00,00,00,00

HKLM,%MediaCategories%\%ADIGUID.CAC3%,Name,,%Control.CAC3%
HKLM,%MediaCategories%\%ADIGUID.CAC3%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%ADIGUID.CPCM%,Name,,%Control.CPCM%
HKLM,%MediaCategories%\%ADIGUID.CPCM%,Display,1,00,00,00,00

[DriverInfo.DelReg]
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%

[DriverInfo.AddReg]
; This section is added to all INFs to add registry entries for Driver Information.
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%,Description,,%DriverDescription%
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%,CurrentVer,,%DriverOEMVersion%
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%,Ver_%DriverOEMVersion%,,%DriverVersionID%
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%, DriverBuildDate,,%DriverBuildDate%
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%, BaseDriverFileName,,"smwdm.sys"
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%, BaseDriverFileVersion,,"5.12.3630"
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%, INFVersion,,%INFVersionID%

[SourceDisksNames]
222=%Empty%,,,

[SourceDisksFiles]
smwdm.sys=222
smwdm4C5.inf=222
migrate.dll=222
a3d.dll=222
smsens.sys=222		;;Sensaura
aeaudio.sys=222		;;Andrea
wdmstub.sys=222		;;wdmstub
;; copy these files into the
;; system32\drivers directory

[WDM_AC97AUD.CopyList]
smwdm.sys
smsens.sys	;;Sensaura
aeaudio.sys	;;Andrea

[Stubfile]		;;wdmstub
wdmstub.sys		;;wdmstub	

[Sensaura]
a3d.dll

;;**************** NT Install ****************

[WDM_JS_JE.NT]
Include=ks.inf,wdmaudio.inf
Needs=Ks.Registration,WDMAUDIO.Registration
CopyFiles=WDM_AC97AUD.CopyList, Sensaura
DelReg=WDM_AC97AUD.DelReg, DriverInfo.DelReg
AddReg=WDM_AC97AUD.AddReg, WDM_AC97AUD_GUID.AddReg, DriverInfo.AddReg, Js_Je.AddReg, Js_JeO.AddReg, SPDIF.AddReg

[WDM_P411.NT]
Include=ks.inf,wdmaudio.inf
Needs=Ks.Registration,WDMAUDIO.Registration
CopyFiles=WDM_AC97AUD.CopyList, Sensaura
DelReg=WDM_AC97AUD.DelReg, DriverInfo.DelReg
AddReg=WDM_AC97AUD.AddReg, WDM_AC97AUD_GUID.AddReg, DriverInfo.AddReg, Js_Je.AddReg, Js_JeP.AddReg, SPDIF.AddReg

[WDM_ASUS.NT]
Include=ks.inf,wdmaudio.inf
Needs=Ks.Registration,WDMAUDIO.Registration
CopyFiles=WDM_AC97AUD.CopyList, Sensaura
DelReg=WDM_AC97AUD.DelReg, DriverInfo.DelReg
AddReg=WDM_AC97AUD.AddReg, WDM_AC97AUD_GUID.AddReg, DriverInfo.AddReg, Js_Je.AddReg, Js_JeA.AddReg, SPDIF.AddReg

[WDM_JS_JE.NT.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%, AC97Aud.Interface.Topology
AddInterface=%ANDREA_INTERFACE%,,AC97Aud.Interface.Andrea

[WDM_P411.NT.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%, AC97Aud.Interface.Topology
AddInterface=%ANDREA_INTERFACE%,,AC97Aud.Interface.Andrea

[WDM_ASUS.NT.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%, AC97Aud.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%, AC97Aud.Interface.Topology
AddInterface=%ANDREA_INTERFACE%,,AC97Aud.Interface.Andrea

; For Andrea

[WDM_JS_JE.NT.HW]
AddReg=FilterAddReg.NT

[WDM_P411.NT.HW]
AddReg=FilterAddReg.NT

[WDM_ASUS.NT.HW]
AddReg=FilterAddReg.NT

;;end Andrea

[AC97Aud.Interface.Wave]
AddReg=AC97Aud.Interface.Wave.AddReg
[AC97Aud.Interface.Wave.AddReg]
HKR,,FriendlyName,,%AC97Aud.Wave.szPname%
HKR,,CLSID,,%Proxy.CLSID%

[AC97Aud.Interface.Topology]
AddReg=AC97Aud.Interface.Topo.AddReg
;;must use topo because topology is too long
[AC97Aud.Interface.Topo.AddReg]
HKR,,FriendlyName,,%AC97Aud.Topology.szPname%

;For Andrea
[AC97Aud.Interface.Andrea]
AddReg=AC97Aud.Interface.Andr.AddReg
[AC97Aud.Interface.Andr.AddReg]
HKR,,FriendlyName,,%AC97Aud.Andrea.szPname%
[FilterAddReg]
HKR,,UpperFilters,0x00010000,AEAudio.sys
[FilterAddReg.NT]
HKR,,"UpperFilters",0x00010000,"AEAUDIO"

[WDM_JS_JE.NT.Services]
AddService = smwdm, 0x00000002, WDM_AC97AUD_Service_Inst
AddService = aeaudio,0x00000000, aeaudio_Service_Inst		;;Andrea

[WDM_P411.NT.Services]
AddService = smwdm, 0x00000002, WDM_AC97AUD_Service_Inst
AddService = aeaudio,0x00000000, aeaudio_Service_Inst		;;Andrea

[WDM_ASUS.NT.Services]
AddService = smwdm, 0x00000002, WDM_AC97AUD_Service_Inst
AddService = aeaudio,0x00000000, aeaudio_Service_Inst		;;Andrea

[WDM_AC97AUD_Service_Inst]
;DisplayName    = %WDM_AC97AUD.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\system32\drivers\smwdm.sys

; For Andrea
[aeaudio_Service_Inst]
;DisplayName    = %AEAudio.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\system32\drivers\aeaudio.sys

[Strings]
;; AC'97 Device friendly names (GUIDS non-localizeable)

ADIGUID.PcBeep      ="{992C6360-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.MonoOut     ="{992C6361-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.Phone       ="{992C6362-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.Video       ="{992C6366-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.PCBeepVol   ="{992C6372-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.MonoVol     ="{992C6374-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.PhoneVol    ="{992C6376-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.VIDVol      ="{992C637A-643D-11D2-9BDC-00A0C9696B7D}"

ADIGUID.20DB        ="{992C6380-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.PHATBypass  ="{992C6387-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.MicSelect   ="{992C638D-643D-11D2-9BDC-00A0C9696B7D}"

ADIGUID.CaptureVid  ="{992C6392-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.CaptureMono ="{992C6396-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.CapturePhone ="{992C6397-643D-11D2-9BDC-00A0C9696B7D}"

ADIGUID.Front       ="{992C636A-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.Surround    ="{992C6365-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.Center      ="{992C6364-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.Lfe         ="{992C6363-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.FrontVol    ="{992C6370-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.SurroundVol ="{992C6381-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.CenterVol   ="{992C6382-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.LfeVol      ="{992C6383-643D-11D2-9BDC-00A0C9696B7D}"
ADIGUID.BBoost      ="{9557C941-7360-11D4-8133-0050046069C0}"
ADIGUID.BBoostVol   ="{9557C942-7360-11D4-8133-0050046069C0}"
ADIGUID.SwapC       ="{A3156CDD-A925-4A37-BD1F-BC9D627F3F06}"
ADIGUID.SwapD       ="{A3156CDE-A925-4A37-BD1F-BC9D627F3F06}"

ADIGUID.CAC3        ="{A3156CD9-A925-4A37-BD1F-BC9D627F3F06}"
ADIGUID.CPCM        ="{A3156CDA-A925-4A37-BD1F-BC9D627F3F06}"

;; Analog Devices friendly names (localizeable)
;Sources (Pins)
Pin.PcBeep       ="PC Beep"          ; PC Beep Input
Pin.MonoOut      ="Mono Out"         ; Mono line output
Pin.Phone        ="Phone"            ; Phone Input
Pin.Video        ="Video"            ; Video Input
Pin.Front        ="Front"            ; Front Output
Pin.Surround     ="Rear"             ; Surround Output
Pin.Center       ="Center"           ; Center Channel Output
Pin.Lfe          ="Subwoofer"        ; Sub woofer ( Lfe )
Pin.BBoost       ="BassBoost"        ; Bass Boost

;Controls       (Controls as related to Sources)

Control.PCBeepVol     ="PCBeep Volume"   ; PC Beep volume control name
Control.PhoneVol      ="Phone Volume"    ; Phone volume control name
Control.VIDVol        ="Video Volume"    ; Video volume control name
Control.20DB          ="MIC Boost"       ; Microphone advanced control
Control.PHATBypass    ="Apply 3D effect to digital audio"
                                         ; 3D bypass control string (bypass
                                         ;  spatialization on digital streams)

Control.MonoVol       ="Mono Volume"     ; Monoaural Output volume control name
Control.MicSelect     ="Front Panel Mic" ; Microphone advanced control

Control.CaptureVid    ="Video"           ; Video Record
Control.CaptureMono   ="Mono Out"        ; Mono Mix Record
Control.CapturePhone  ="Phone"           ; Phone Record

Control.FrontVol     ="Front Volume"     ; Front Output
Control.SurroundVol  ="Rear Volume"      ; Surround Output
Control.CenterVol    ="Center Volume"    ; Center Channel Output
Control.LfeVol       ="Subwoofer Volume" ; Sub woofer ( Lfe )
Control.BBoostVol    ="BassBoost Level"  ; Bass Boost
Control.SwapC        ="Swap Center/Subwoofer"
Control.SwapD        ="Swap Center/Subwoofer Data"

Control.CAC3	     ="AC3 SPDIF"	 ; AC3 Select
Control.CPCM	     ="PCM SPDIF"	 ; PCM Select

MediaCategories="SYSTEM\CurrentControlSet\Control\MediaCategories"
Upgd="Software\Microsoft\Windows\CurrentVersion\Setup\UpgradeDrivers"
UpDir="win9xmig\DevUpgrd\ADIW2K\smwdm4C5.inf"
WDM_MIDI="WDM-based Device"
Proxy.CLSID="{17CCA71B-ECD7-11D0-B908-00A0C9223196}"
KSCATEGORY_AUDIO="{6994AD04-93EF-11D0-A3CC-00A0C9223196}"
KSCATEGORY_RENDER="{65E8773E-8F56-11D0-A3B9-00A0C9223196}"
KSCATEGORY_CAPTURE="{65E8773D-8F56-11D0-A3B9-00A0C9223196}"
KSNAME_Wave="Wave"
KSNAME_Topology="Topology"
ANDREA_INTERFACE="{56907941-3AFE-11d4-AE2C-00A0CC242D2C}"
AC97Aud.Andrea.szPname="Andrea in SoundMAX"

ANLG="Analog Devices"
MfgName="Analog Devices, Inc."
Empty="Install disk"

*WDM_AC97AUD.DeviceDesc="SoundMAX Integrated Digital Audio"
AC97Aud.Wave.szPname="SoundMAX Digital Audio"
AC97Aud.Topology.szPname="SoundMAX Digital Audio"

;WDM_AC97AUD.SvcDesc = "SoundMAX Integrated Digital Audio"

; History Information
DriverMfgr="AnalogDevices"
DriverVersionID="5.12.3630"
DriverBuildDate="06/02/2003"
DriverBuildID="5.12.01.3630"
INFVersionID="5.12.01.3630-0005"
DriverOEM="AnalogDevices"
DriverFamily="Audio"
DriverProduct="SoundMAX"
DriverDescription="Audio Driver"
DriverOEMVersion="x00"

